Specifications text



Article number
226673

Type
SeeEyes SC-IPE3001

Short description
Ethernet, PoE Extender, UTP, 1 Port, extension 100m, 250m max., PoE injector

Main Features
Extension of the Ethernet range up to 250m
Bandwidth 10/100Mbps full duplex
Distance 100Mbps: max. 100m(CAT.5e)
Distance 10Mbps: max. 250m(CAT.5e)
Operating temperature -10°C~+50°C
PSU included

Other Features (Specifications)
	General
	

	Type
	PoE Extender

	Temperature Range (Operating)
	-10°C ~ +50°C

	Interfaces / Inputs/ Outputs
	

	PoE Standard
	PoE (IEEE802.3af)

	Ports
	1

	 Product labeling:
	

	Manufacturer order number
	SC-IPE3001

	Series
	SeeEyes SC-IP

	Brand
	SeeEyes
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