Specifications text



Article number
237251

Type
SeeEyes SC-IPU601R

Short description
1-channel-IP receiver, PoE over UTP, High Power (70W) , High Reach up to 800m

Main Features
1-channel IP + PoE via UTP receiver
PoE++ (IEEE 802.3af/at/bt, max 70W
Transmission range: 100Mbps up to 500m
Transmission range: 10Mbps to 800m
Supports Auto MDI/MDIX function
Power transmission with automatic power diagnostics
Built-in overvoltage protection
Power supply included

Other Features (Specifications)
	General
	

	Design
	Module

	Type
	Media converter

	Mounting type
	Wall

	PoE Budget (Total)
	70 W

	Reach
	800 km

	Power supply
	56VDC, Poe

	Temperature Range (Operating)
	-10°C ~ +50°C

	Interfaces / Inputs/ Outputs
	

	Ports
	1

	 Product labeling:
	

	Manufacturer order number
	SC-IPU601R + 56V 2A

	Series
	SeeEyes SC-IP

	Brand
	SeeEyes



Additional Productinformation



Related products

Recommendations

Services
	SeeEyes SC-IPU601T
	1-channel-IP transmitter PoE over UTP, High Power (70W), High Reach up to 800m


