Specifications text



Article number
246625

Type
eneo IND-42M2808M0A

Short description
Mini Network Dome Camera Fix, 1920x1080, Day/Night, WDR, AI 2,8-8mm, IR, 12VDC, PoE, IP66, IK10

Main Features
1/2.8" Sony STARVIS CMOS sensor,2 MP/60fps
AI analysis functions including object classification
WDR 120dB, 3D-DNR Noise Reduction
Motorized varifocal lens 2.8-8mm
Smart Codec H.265/H.264, multi-streaming
Browser independent (IE, Edge, Safari, Firefox, Chrome)
Supports ONVIF profiles S/T/G/M
Multilingual menu navigation (OSD)
Local storage via Micro SD card
Supports audio and external alarm input and output
NDAA compliance
IR LED illumination, IP66 and vandal proof IK10

Other Features (Specifications)
	Other
	

	EAN/GTIN
	4260229841846

	Analysis
	Crowds (CD), Enter Region, Face Recognition (FR), Heat Map (HM), Intrusion, Leave Region, License plate recognition (LPR), Line crossing (LCD), Object Classification Human / Vehicle (PD&VD), Passage count (CC), Queues (QD), Rare Sounds (RSD)

	Audio support
	Yes

	Motion detector
	Yes

	Digital Noise Reduction (DNR)
	Yes

	Multicast
	Yes

	Backlight compensation
	Yes

	Low Speed Shutter
	Yes

	Vandalism-resistant
	Yes

	Alarm inputs
	1

	Audio compression
	G.711

	Resolution standard
	2 MP

	Recording sensor
	CMOS, SC235HAI, SSC30KQ

	Lighting
	Infrared

	Image resolution max.
	1920x1080

	Image transfer rate max.
	60 fps

	Horizontal angle of view
	100 - 44°

	Vertical angle of view
	56 - 25°

	Focal length
	2,8 - 8 mm

	Chip size
	1/2,9"

	Turning range
	350 °

	Dimensions (WxHxD) (extended)
	115x91,6mm

	Alarm processing
	Recording internal storage (SD card),E-Mail,HTTP,FTP,TCP,UDP,alarm out,Cloud Upload

	Audio
	2 Way Audio

	Resolution (extended)
	1920x1080 (16:9),1280x960 (4:3),1280x720 (16:9),640x480 (4:3),320x240 (4:3)

	Illumination range
	Approx. 20m

	Remark
	Face and license plate recognition require an SD card or an eneo IN recorder. For optimal results,use only eneo components. For mixed brands,we offer a compatibility check for a fee (info: item #229235 at VIDEOR).

	Watch (62px/m)
	13,9 - 38,7m

	Picture size
	16:9, 4:3

	Aperture Range (F)
	F1.8

	Browser
	Edge, Firefox, Google Chrome, MS Internet Explorer 10/11, Safari

	Data stream types
	Triple-Stream(Main/Sub/Mobile)

	Detect (125px/m)
	5,5 - 18,7m

	ESC
	1/5 ~ 1/20.000sec.

	External connections
	RJ-45,Alarm in/output,Audio input/output,12VDC input (DC plug),connection cable approx.45cm,micro SD card slot 512 GB

	Flickerless function
	Yes

	Weight
	0.56 kg

	Identify (250px/m)
	2,7 - 8,6m

	Camera shape
	Minsters

	Scope of delivery
	Quick installation guide,drilling template,4 wall plugs with screws,1 Torx wrench,waterproof cover for RJ45 connector

	Manual Electric Shutter (MES)
	1-5~1-20,000sec.

	Menu languages
	English, French, German, Italian, Japanese, Portuguese, Spanish, Turkish

	Password
	Administrator and User

	Privacy Zone
	Areas-ON/OFF switchable

	SDK
	Upon request

	Security
	Complicated password, IP address filtering, Password

	Signal-to-noise ratio
	41 dB

	Day/night mode
	Automatic,Day,Night,Image,Time

	Text overlay
	Switchable on/off

	Vertical tilt range
	0~ +80°

	Perceiving (25px/m)
	37,3 - 96,9m

	White balance
	Automatic,Manual

	Ethernet interface
	100Base-TX, 10Base-T

	Color (Housing)
	RAL9003,Other colors available upon request

	Color (dome)
	clear

	Housing type
	Outside

	Housing material
	Aluminium

	Internal memory
	microSD card slot

	Camera Type
	Domecamera

	Power consumption
	6.2 W

	Photosensitivity
	Color 0,0034lux bei F1.6(AGC ON)

	MOD (Minimum Object Distance)
	0.8 m

	Mounting type
	Ceiling, Wall

	Network Protocols
	DDNS, DHCP, DNA, FTP, HTTP, HTTPS, NTP, RTP, RTSP, SMTP, TCP-IP, UPnP

	Lens Type
	Varifocal (motorized)

	ONVIF
	ONVIF Profile G, ONVIF Profile M, ONVIF Profile S, ONVIF Profile T

	Manufacturer order number
	246625

	Power over Ethernet
	IEEE 802.3af

	Protection
	IP67

	Series
	eneo IN-Serie

	Control Interfaces
	Ethernet

	Power supply
	12VDC, Poe

	System
	True Day&Night

	Day/night switching
	Switchable IR Filter (ICR)

	Temperature Range (Operating)
	-35°C ~ +60°C,@ Luftfeuchtigkeit 90% oder weniger (nicht kondensierend)

	Video Compression
	H.264, H.264+, H.265, H.265+, MJPEG

	Wide Dynamic Range (WDR)
	120dB

	Certifications
	IK10

	Zoomfactor (optical)
	3

	Brand
	eneo



Additional Productinformation



Related products
	eneo AK-22
	Camera junction box for wall and ceiling mount, Mini Dome IND-42M2808M0A

	eneo AK-23
	Camera connection box for Mini Dome IND-42M2808M0A for holder Dome-WB6/Dome-CH6

	eneo DOME-WB7
	Wall bracket for Mini Dome IND-42M2808M0A

	eneo INsight
	Control software for recorder IN- and MN-series

	eneo INsight Installation Tool
	Supports adjustments for cameras with AI features for IN-series

	eneo INsight mobile
	Mobile App for recorder IN- and MN-series

	eneo Site Manager
	Management Software for eneo IP products



Recommendations
	eneo NSMI-4004M0A
	Gigabit Switch Industrial, Managed, 4x PoE, 2xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSMI-4008M0A
	Gigabit Switch Industrial, Managed, 8x PoE, 2xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSMR-2008M0A
	Gigabit Switch Rack, Managed, 8x PoE, 2xSFP, max. 30W each Port, internal Power Supply max. 150W

	eneo NSMR-2016M0A
	Gigabit Switch Rack, Managed, 16x PoE, 2xSFP, max. 30W each Port, integrated Power Suppply max. 250W

	eneo NSMR-2024M0A
	Gigabit Switch Rack, Managed, 24x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 400W

	eneo NSUI-3004M0A
	Gigabit Switch Industrial, Unmanaged, 4x PoE, 1xRJ45, 1xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSUI-3008M0A
	Gigabit Switch Industrial, Unmanaged, 8x PoE, 2xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSUR-1008M0A
	Gigabit Switch Rack, Unmanaged, 8x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 150W

	eneo NSUR-1016M0A
	Gigabit Switch Rack, Unmanaged, 16x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 250W

	eneo NSUR-1024M0A
	Gigabit Switch Rack, Unmanaged, 24x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 400W

	jetrics jetcat6SFTP-GN-0,5/1
	

	jetrics jetcat6SFTP-GN-1/1
	

	jetrics jetcat6SFTP-GN-2/1
	

	jetrics jetcat6SFTP-GN-3/1
	

	jetrics jetcat6SFTP-GN-7,5/1
	

	jetrics jetpower-PSU-XS-11C Steckernetzteil
	



Services
	PAINTING SERVICE basic costs
	once per RAL color and delivery lot

	PAINTING SERVICE fix dome camera
	in RAL color

	Vorkonfiguration IP-Kamera
	Preconfiguration 1x IP camera Function test, FW update


