Specifications text



Article number
246665

Type
eneo IND-58F0002MTPB

Short description
Network Dome Camera Fix, Turret, Panorama 180°, 2x 5120x1440, Day/Night, DWDR, AI, 2x 2,8mm, IR, White Light, 12VDC, PoE, IP67

Main Features
Multisensor 2x 1/2.7’ CMOS sensor, panorama
Maximum resolution 5120x1440 pixels each, 15fps
Panorama ultra wide-angle camera 180° HFoV, 32:9
AI analysis functions including object classification
WDR, BLC, HLC and 3D-DNR noise reduction
Lenses with 2.8mm fixed focal length
Smart Codec H.265/H.264, dual streaming
Browser-independent (Edge, Safari, Firefox, Chrome)
Supports ONVIF profiles S/T/G/M and audio
Local storage via micro SD card
NDAA compliance
Integrated IR and white light LED illumination, IP67

Other Features (Specifications)
	Other
	

	EAN/GTIN
	4260229841884

	Analysis
	Crowds (CD), Enter Region, Face, Heat Map (HM), Intrusion, Leave Region, License plate recognition (LPR), Line crossing (LCD), Object classification, Object Classification Human / Vehicle (PD&VD), People counting, Queues (QD), Rare Sounds (RSD)

	Audio support
	Yes

	Motion detector
	Yes

	Digital Noise Reduction (DNR)
	Yes

	Multicast
	Yes

	Backlight compensation
	Yes

	Low Speed Shutter
	Yes

	Audio compression
	G.711a, G.711u

	Resolution standard
	8 MP

	Recording sensor
	Chipset NT98529, CMOS, SC533HAI

	Lighting
	Infrared, Warm Light

	Image resolution max.
	5120x1440

	Image transfer rate max.
	15 fps

	Horizontal angle of view
	180°

	Vertical angle of view
	60°

	Focal length
	2,8 mm

	Chip size
	1/2,7"

	Dimensions (WxHxD) (extended)
	112,4x135 mm

	Alarm processing
	Recording internal storage (SD card),E-Mail,HTTP,FTP,TCP,UDP,Red & bule flashing lights,Cloud Upload

	Audio
	2 Way Audio, Built-in microphone, Built-in speaker

	Resolution (extended)
	5120x1440,4608x1296,4096x1152,3840x1080,3072x864,1536x432,1024x288

	Illumination range
	Approx. 30 m | Approx. 15 m Warm light 

	Remark
	Face and license plate recognition require an SD card or an eneo IN recorder. For optimal results,use only eneo components. For mixed brands,we offer a compatibility check for a fee (info: item #229235 at VIDEOR).

	Watch (62px/m)
	23,8m

	Aperture Range (F)
	F1,2

	Browser
	Edge, Firefox, Google Chrome, MS Internet Explorer 10/11, Safari

	Data stream types
	Dual Streaming

	Detect (125px/m)
	11,7m

	ESC
	1/5 ~ 1/20.000sec.

	External connections
	RJ-45,12VDC input (DC plug),connection cable approx.30cm,micro SD card slot 256 GB

	Flickerless function
	Yes

	Weight
	0.765 kg

	Identify (250px/m)
	5,5m

	Camera shape
	Minsters

	Scope of delivery
	Quick installation guide,drilling template,3x wall plugs with screws,1x Allen wrench,1x waterproof cover for RJ45 connector

	Manual Electric Shutter (MES)
	1-5~1-20,000sec.

	Menu languages
	English, French, German, Italian, Japanese, Portuguese, Spanish, Turkish

	Password
	Administrator and User

	Privacy Zone
	Areas-ON/OFF switchable

	SDK
	Upon request

	Security
	Complicated password, HTTPS encryption, IP address filtering, Password

	Signal-to-noise ratio
	49 dB

	Day/night mode
	Day,Night,Automatic,Time

	Text overlay
	Switchable on/off

	Perceiving (25px/m)
	60,1m

	White balance
	Automatic,Manual

	Ethernet interface
	100Base-TX, 10Base-T

	Color (Housing)
	RAL9003,Other colors available upon request

	Housing type
	Outside

	Housing material
	Aluminium

	Internal memory
	microSD card slot

	Camera Type
	Panoramic camera

	Power consumption
	13.5 W

	Photosensitivity
	0.001 Lux bei (F1.6,AGC ON)

	MOD (Minimum Object Distance)
	2 m

	Mounting type
	Ceiling, Wall

	Network Protocols
	DDNS, DHCP, DNA, FTP, HTTP, HTTPS, IPv4, IPv6, NTP, PPPoE, RTP, RTSP, SMTP, TCP-IP, UPnP, UTP

	Lens Type
	Prime lens

	ONVIF
	ONVIF Profile G, ONVIF Profile M, ONVIF Profile S, ONVIF Profile T

	Manufacturer order number
	246665

	Power over Ethernet
	IEEE 802.3af

	Protection
	IP67, NEMA 4X

	Series
	eneo IN-Serie

	Control Interfaces
	Ethernet

	Power supply
	12VDC, Poe

	System
	True Day&Night

	Day/night switching
	Switchable IR Filter (ICR)

	Temperature Range (Operating)
	-30°C ~ +60°C,@ Luftfeuchtigkeit 90% oder weniger (nicht kondensierend)

	Video Compression
	H.264, H.264+, H.265, H.265+, MJPEG

	Wide Dynamic Range (WDR)
	WDR 120dB

	Brand
	eneo



Additional Productinformation



Related products
	eneo AK-20
	Camera connection box for Wall and ceiling mounting, IN Series Bullet Cameras

	eneo AK-21
	Camera connection box for Wall and ceiling mounting, Bullet and Dome Cameras IN series

	eneo AK-24
	Dual camera connection box for selected Bullet or Fix Dome IN-Series cameras

	eneo DOME-WB8
	Wall bracket for PTZ dome INP-54M2812M0A and IND-5 Dome Series

	eneo INsight
	Control software for recorder IN- and MN-series

	eneo INsight Installation Tool
	Supports adjustments for cameras with AI features for IN-series

	eneo INsight mobile
	Mobile App for recorder IN- and MN-series

	eneo Site Manager
	Management Software for eneo IP products



Recommendations
	eneo NSMI-4004M0A
	Gigabit Switch Industrial, Managed, 4x PoE, 2xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSMI-4008M0A
	Gigabit Switch Industrial, Managed, 8x PoE, 2xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSMR-2008M0A
	Gigabit Switch Rack, Managed, 8x PoE, 2xSFP, max. 30W each Port, internal Power Supply max. 150W

	eneo NSMR-2016M0A
	Gigabit Switch Rack, Managed, 16x PoE, 2xSFP, max. 30W each Port, integrated Power Suppply max. 250W

	eneo NSMR-2024M0A
	Gigabit Switch Rack, Managed, 24x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 400W

	eneo NSUI-3004M0A
	Gigabit Switch Industrial, Unmanaged, 4x PoE, 1xRJ45, 1xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSUI-3008M0A
	Gigabit Switch Industrial, Unmanaged, 8x PoE, 2xSFP, 30W each Port, -40°C~75°C, 44~57 VDC, w/o power supply

	eneo NSUR-1008M0A
	Gigabit Switch Rack, Unmanaged, 8x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 150W

	eneo NSUR-1016M0A
	Gigabit Switch Rack, Unmanaged, 16x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 250W

	eneo NSUR-1024M0A
	Gigabit Switch Rack, Unmanaged, 24x PoE, 2xSFP, max. 30W each Port, integrated Power Supply max. 400W

	jetrics jetcat6SFTP-GN-0,5/1
	

	jetrics jetcat6SFTP-GN-1/1
	

	jetrics jetcat6SFTP-GN-2/1
	

	jetrics jetcat6SFTP-GN-3/1
	

	jetrics jetcat6SFTP-GN-7,5/1
	

	jetrics jetpower-PSU-XS-11C Steckernetzteil
	



Services
	PAINTING SERVICE basic costs
	once per RAL color and delivery lot

	PAINTING SERVICE fix dome camera
	in RAL color

	Vorkonfiguration IP-Kamera
	Preconfiguration 1x IP camera Function test, FW update


