Specifications text



Article number
247579

Type
Solvido SOL-IQbox-budget-B/Hz

Short description
Camera junction box for video surveillance incl. heating, 400x300x150mm

Main Features
Optimised for outdoor use
With extended temperature range
Electrically prewired for flexible, modular expansion.
UV stable polycarbonate, corrosion-resistant
Protective class IP66,
Impact resistance IK 10, vandalism protected
Swivelling door
Wall or mast mounted
Fast, easy installation
Simple mechanical finishing

Other Features (Specifications)
	Other
	

	Color (Housing)
	RAL7035

	Housing material
	Polycarbonate

	Installation Location
	Outdoor

	Mounting type
	Mast mounting, Wall

	Manufacturer order number
	247579

	Protection
	IP66

	Series
	Solvido IQbox

	Power supply
	230VAC

	Temperature Range (Operating)
	-40°C ~ +80°C

	Certifications
	IK10

	Brand
	Solvido



Additional Productinformation



Related products
	jetrics MDR-100-12
	Power Supply 12V / 7,5A for DIN rail mounting TS-35

	jetrics MDR-100-48
	Power Supply 48V / 2A

	jetrics MDR-20-12
	Power Supply 12VDC / 1,67A for DIN rail mounting TS-35

	jetrics MDR-60-12
	Power Supply 12VDC / 5A for DIN rail mounting TS-35

	jetrics MDR-60-48
	Power Supply 48VDC / 1,25A for DIN rail mounting TS-35

	jetrics NDR-120-48 DIN Rail
	Power Supply, 230VAC / 48VDC, max. 120W, for DIN rail mounting

	jetrics NDR-240-48 DIN RAIL
	Power Supply, 230VAC / 48VDC, max. 240W, for DIN rail mounting

	Solvido 50W Semiconductor power supply
	with thermostat, for DIN rail mounting

	Solvido SOL-WST-MB-30
	Pole mounting for CUS-WST and SOL-IQbox series set (2pcs)

	Solvido SOL-WST-SSK-ES-30
	

	Solvido SOL-WST-SSK/1
	Lock with toggle lock (1 piece) with key, for CUS-WST and SOL-IQbox series

	Solvido SOL-WST-WB
	Wall mounting for CUS-WST and SOL-IQbox series set (4pcs) wall clearance 10mm



Recommendations

Services
