Specifications text



Article number
219643

Type
eneo MAM-6ME1012MTA

Short description
Multisignal Converter, HD-TVI , AHD, CVBS to IP, H.264, 1920x1080, 12-Channel

Main Features
Multisignal converter HD-TVI, AHD, CVBS to IP
Automatic signal and resolution detection
Resolution max. 1920x1080 (Full HD)
Compression H.264, audio support
Multi and single screen support
HDMI, VGA Main and CVBS Spot monitor output
PTZ control via RS-485 and UTC
Motion controller, alarm inputs and output
Menu control via USB mouse (optional)
LED status display
Compatible with eneo Center CMS

Other Features (Specifications)
	General
	

	Dimensions (WxHxD) (extended)
	44.9x375x318.2mm

	Weight
	1.8 kg

	Color (Housing)
	Black

	Housing material
	Aluminium, Plastic

	Installation Location
	Indoor

	Power consumption
	13.5 W

	Mounting type
	19" Rack Installation, Desktop

	Power supply
	12VDC

	Temperature Range (Operating)
	0°C ~ +45°C

	Parts supplied
	

	Scope of delivery
	QIG,power supply unit,19\" rack-mount brackets

	 Product labeling:
	

	Manufacturer order number
	219643

	Series
	eneo COAXIZE

	Brand
	eneo



Additional Productinformation



Related products

Recommendations
	jetrics cable BNC BS-BS-1
	Videokabel mit 2 x BNC-Stecker 1m, 75 Ohm

	jetrics cable BNC BS-BS-2
	Videokabel mit 2 x BNC-Stecker 2m, 75 Ohm

	jetrics cable BNC BS-BS-3
	Videokabel mit 2 x BNC-Stecker 5m, 75 Ohm

	jetrics cable BNC BS-BS-3
	Videokabel mit 2 x BNC-Stecker 3m, 75 Ohm

	jetrics jetpower-PSU-XS-11C Steckernetzteil
	



Services
