Specifications text



Article number
221811

Type
SeeEyes SC-IPM07PRO

Short description
7" (17,8cm) Test Monitor, Touch, IP, HD/3G/EX-SDI, TVI, CVI, AHD, Composite, HDMI

Main Features
7" touch monitor for setup and service
Imputs: IP, HD/3G/EX-SDI, TVI/CVI/AHD, CVBS
AHD/TVI/CVI up to 8 megapixels
HDMI input/output
Resolution: 1920x1200 pixels
SFP-Port single-mode, multi-mode
IP address scan and search, ping test, link test
Cable tester for coax and UTP
12VDC power supply for camera
Li-Polymer battery
Carry-on case inclused

Other Features (Specifications)
	General
	

	Power supply
	12VDC

	Temperature Range (Operating)
	0°C ~ +50°C

	Video
	

	Video Compression
	H.264, H.265, M-JPEG

	 Product labeling:
	

	Manufacturer order number
	SC-IPM07PRO

	Brand
	SeeEyes



Additional Productinformation



Related products
	SC BATTERY LARGE
	Akku für Multiformat SeeEyes Servicemonitor, groß, Ersatzteil ab 08/17

	SeeEyes SC-Charger (12.6V)
	Netzteil für Multiformat Servicemonitore, Ersatzteil



Recommendations

Services
