Specifications text



Article number
226671

Type
SeeEyes SC-IPC07P

Short description
Media Converter Set, 1 Channel Ethernet over Coax Transmitter Receiver, Transmission 1000m

Main Features
1-channel Ethernet via coax transmission
Set consisting of transmitter and receiver
Long distance transmission via RG-6
Transmission range: 100Mbps up to 500m
Transmission range: 10Mbps up to 1km
Power supply unit included

Other Features (Specifications)
	General
	

	Design
	Mini module

	Type
	Media converter

	Mounting type
	Wall

	Reach
	1 km

	Power supply
	48VDC, Poe

	Temperature Range (Operating)
	-10°C ~ +50°C

	Interfaces / Inputs/ Outputs
	

	Ports
	1

	 Product labeling:
	

	Manufacturer order number
	SC-IPC07P

	Series
	SeeEyes SC-IP

	Brand
	SeeEyes
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