Specifications text



Article number
236267

Type
SeeEyes SC-HLR01P

Short description
HD-SDI repeater up to 200m (1.5G), PoC, 12VDC

Main Features
HD-SDI Signal Repeater
Range extension up to 200 m (HD:1.5G) via RG-6
150 m via RG-59
Power supply via coaxial (PoC)
Power supply: 12VDC

Other Features (Specifications)
	General
	

	Design
	Mini module

	Type
	Repeater

	Power supply
	12VDC

	Temperature Range (Operating)
	-10°C ~ +50°C

	Interfaces / Inputs/ Outputs
	

	Ports
	1

	 Product labeling:
	

	Manufacturer order number
	SC-HLR01P

	Brand
	SeeEyes
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