Specifications text



Article number
236811

Type
SeeEyes SC-IPC0708H

Short description
Mediaconverter set, 8-channel, Ethernet over Coax, reach 1000m

Main Features
8-channel Ethernet via coax transmission
Set consisting of transmitter and receiver (hub)
Long distance transmission via RG-6
Transmission range: 100Mbps up to 500m
Transmission range: 10Mbps up to 1km
Power supply unit included

Other Features (Specifications)
	General
	

	Design
	Mini module, Module

	Type
	Media converter

	Mounting type
	Wall

	Reach
	1 km

	Power supply
	240VAC, Poe

	Temperature Range (Operating)
	-10°C ~ +50°C

	Interfaces / Inputs/ Outputs
	

	Ports
	1, 8

	 Product labeling:
	

	Manufacturer order number
	SC-IPC0708H

	Series
	SeeEyes SC-IP

	Brand
	SeeEyes



Additional Productinformation



Related products

Recommendations

Services
