Specifications text



Article number
236813

Type
SeeEyes SC-IPC1201TW

Short description
2-wire IP transmission set PoE, 700m reach 48V power supply included

Main Features
2-wire IP transmission set
Range with TP cable up to 700m / T-cable 200m
Power transmission via PoE
Overvoltage protection integrated
48V power adapter included

Other Features (Specifications)
	General
	

	Type
	Receiver, Transmitter

	Temperature Range (Operating)
	-10°C ~ +50°C

	Interfaces / Inputs/ Outputs
	

	PoE Standard
	PoE+ (IEEE802.3at)

	Ports
	1

	 Product labeling:
	

	Manufacturer order number
	SC-IPC1201TW + 56V 2A Powersupply

	Series
	SeeEyes SC-IP

	Brand
	SeeEyes
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