Specifications text



Article number
218800

Type
SeeEyes SC-IPC3001E

Short description
Media Converter Set, 1 Channel Ethernet over Coax Transmitter Receiver, PoE 1,8km

Main Features
1-Channel Ethernet over Coax Transmission
Transmitter and Receiver Set
Bandwidth: 200 Mbps
Transmission Distance: 1,800 m via RG-6
Button for automatic pairing
Transmitter supports PoE output for camera
48 VDC power supply included

Other Features (Specifications)
	General
	

	Design
	Mini module

	Type
	Media converter

	Mounting type
	Wall

	Reach
	1,800 km

	Power supply
	48-56VDC

	Temperature Range (Operating)
	-10°C ~ +50°C

	Interfaces / Inputs/ Outputs
	

	Ports
	1

	 Product labeling:
	

	Manufacturer order number
	SC-IPC3001E

	Brand
	SeeEyes
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